SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( VR2N_Bx_NPDC
	Type ( Carriage )
	WagonShape ( VR2N_Bx_NPDC.s )

	Size ( 2.82m 4.3m 24.09m )
	CentreOfGravity ( 0.0m 1.0m 0.0m )
	Mass ( 51t )
	InertiaTensor ( Box (2.82m 4.3m 24.09m) )
	Coupling (
		Type ( Chain )
		Spring (
			Stiffness ( 1e6N/m 2e6N/m )
			Damping ( 1e6N/m/s 1e6N/m/s)
			Break ( 1e7N 1e7N )
			r0 ( 10cm 40cm )
		)
		CouplingHasRigidConnection ()
		Velocity ( 0.1m/s )
	)
	Buffers (
		Spring (
			Stiffness ( 5e6N/m 5e6N/m )
			Damping ( 1e6N/m/s 1e6N/m/s )
			r0 ( 0m 1e9 )
		)
		Centre ( 0.5 )
		Radius ( 1 )
		Angle ( 0.5deg )
	)
	Inside (
          PassengerCabinFile ( Cabine_VR2n.s	)
           PassengerCabinHeadPos ( 0.6 2.6 -11.2 )
           RotationLimit ( 60 360 0 )
           StartDirection ( 7 180 0 )
           Sound ( "VO2Npas.sms" )
	  
      )
      Lights	(	4

		Light	(
			comment( fanal arriere gauche )
			Type		( 0 )
			Conditions	(
				Headlight ( 1 )  
				Unit ( 3 )
			)
			Cycle		( 0 )
			States	(	1
				State	(
					Duration ( 0 )
					LightColour ( ffffffff )
					Position ( 0.955 1.702 -11.9 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)

		Light	(
			comment( fanal arriere droit )
			Type		( 0 )
			Conditions	(
				Headlight ( 1 )  
				Unit ( 3 )
			)
			Cycle		( 0 )
			States	(	1
				State	(
					Duration ( 0 )
					LightColour ( ffffffff )
					Position ( -0.955 1.702 -11.9 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)

		Light	(
			comment( fanal arriere gauche 2 )
			Type		( 0 )
			Conditions	(
				Headlight ( 2 )  
				Unit ( 3 )
			)
			Cycle		( 0 )
			States	(	1
				State	(
					Duration ( 0 )
					LightColour ( ffff2211 )
					Position ( 0.68 1.702 -11.9 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.4 )
				)
			)
		)

		Light	(
			comment( fanal arriere droit 2 )
			Type		( 0 )
			Conditions	(
				Headlight ( 2 )  
				Unit ( 3 )
			)
			Cycle		( 0 )
			States	(	1
				State	(
					Duration ( 0 )
					LightColour ( ffff2211 )
					Position ( -0.68 1.702 -11.9 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.4 )
				)
			)
		)
	)
	BrakeEquipmentType( "Handbrake, Triple_valve, Auxilary_reservoir, Emergency_brake_reservoir" )
	BrakeSystemType( "Air_single_pipe" )
	MaxBrakeForce( 50kN )

	MaxHandbrakeForce( 35kN )
	EmergencyBrakeResMaxPressure( 70 )
	TripleValveRatio( 2.5 )
	MaxReleaseRate( 20 )
	MaxApplicationRate( 20 )
	MaxAuxilaryChargingRate( 25 )
	EmergencyResCapacity( 14 )
	EmergencyResChargingRate( 18 )
	BrakeCylinderPressureForMaxBrakeBrakeForce( 50 )

	Adheasion ( 0.2 0.4 2 0 )
	DerailRailHeight ( 4cm )
	DerailRailForce ( 2.5*41.000t )
	DerailBufferForce ( 1000kN )
	WheelRadius ( 0.4m )
	NumWheels (	8 )
	Friction (
		50N/m/s			1		-1mph		0		1
		5.1N/rad/s		1		-1rad/s		0		1
	)

	Sound ( "XBXEPiloteeng.sms" )


)
